


1. Please Un-compress the SecureModeUpgrade.rar. There will be five files in the uncompressed folder as below screenshot. Running tool of **StartHere.exe**  
   ****
2. Please modify the IP of the PC to 192.168.1.200  
   
3. Connect PC and the phone use one cable.  
   
4. Please Keep pressing ‘\*’ and ‘1’ keys and start up the phone until the LCD displays Upgrading information;
5. the phone will download the **Kernel** from the PC. Wait for about five minutes. After the download is done, the phone will upgrade automatically.

Note: after upgrade the files, sometimes the phone would auto restart about 5 times, please also wait for it.